> ## Specifications

> - Software Features
> - Hardware Specifications
> - Available Channels

> ## Software Features

> The tables below list the software features available on the AP-4000 Series.

> - Number of Stations per BSS
> - Management Functions
> - Advanced Bridging Functions
> - Medium Access Control (MAC) Functions
> - Security Functions
> - Network Functions

> ## Number of Stations per BSS

> Feature | Supported by AP-4000 Series
> Without encryption | up to 63
> With WEP encryption | up to 63
> With 802.1x Authentication | up to 63
> With WPA | up to 27
> With 802.11i (WPA2) | up to 63

> ##

> ## Management Functions

> Feature | Supported by AP-4000 Series
> Web User Interface | 3
> Telnet / CLI | 3
> SNMP Agent | 3
> Serial CLI | 3
> Secure Management | 3
> SSH | 3
> RADIUS Based Management Access | 3

> ##

> ## Advanced Bridging Functions

> Feature | Supported by AP-4000 Series
> IEEE 802.1d Bridging | 3
> WDS Relay | 3
> Roaming | 3
> Protocol Filtering | 3
> Multicast/Broadcast Storm Filtering | 3
> Proxy ARP | 3
> TCP/UDP Port Filtering | 3
> Blocking Intra BSS Clients | 3
> Packet Forwarding | 3

> ##

> ## Medium Access Control (MAC) Functions

> Feature | Supported by AP-4000 Series
> Automatic Channel Selection (ACS) | 3
> Dynamic Frequency Selection (DFS)/Radar Detection (RD)* | 3
> Wireless Service Shutdown | 3
> 802.11d Support | 3
> TX Power Control | 3
> Wireless Multimedia Enhancements/Quality of Service (QoS) | 3
> Channel Blacklist | 3
> Closed System | 3
> Broadcast SSID | 3
> Super and Turbo Mode Support | 3

> ##

> * DFS is required for 802.11a APs certified in the ETSI and TELEC regulatory domains and operating in the middle frequency band. When ACS is disabled, available channels are limited to those in the lower frequency band. See Dynamic Frequency Selection/Radar Detection (DFS/RD).

> ## Security Functions

> Feature | Supported by AP-4000 Series
> Security Profiles per VLAN | 3
> RADIUS Profiles per VLAN | 3
> IEEE 802.11 WEP* | 3
> MAC Access Control | 3
> RADIUS MAC-based Access Control | 3
> IEEE 802.1x Authentication† | 3
> Multiple Authentication Server Support per VLAN‡ | 3
> Rogue Scanning to Detect Rogue Access Points and Clients | 3
> Per User Per Session (PUPS) Encryption § | 3
> Wi-Fi Protected Access (WPA)/802.11i (WPA2) | 3
> Hardware Configuration Reset Disable | 3

> ##

> * Key lengths supported by 802.11a: 64-bit, 128-bit, and 152-bit.
> Key lengths supported by 802.11b: 64-bit and 128-bit.
> Key lengths supported by 802.11b/g: 64-bit, 128-bit, and 152-bit.
> † EAP-MD5, EAP-TLS, EAP-TTLS, and PEAP client supplicant supported.
> ‡ Support is provided for a primary and backup RADIUS authentication server for both MAC-based authentication and 802.1x authentication per VLAN.
> § Use in conjunction with WPA or 802.1x Authentication.

> ## Network Functions

> Feature | Supported by AP-4000 Series
> DHCP Client | 3†
> DHCP Server | 3†
> DHCP Relay Agent and IP Lease Renewal | 3
> Inter Access Point Protocol (IAPP) | 3
> Link Integrity | 3
> System Logging (Syslog) | 3
> RADIUS Accounting Support* | 3
> DNS Client | 3
> TCP/IP Protocol Support | 3
> Virtual LAN Support | Up to 16 SSIDs and VLANs per wireless interface, with specific Security and RADIUS profiles. For more information, see the Advanced Configuration chapter.
> Mesh Networking | 3‡

> ##

> * Includes Fallback to Primary RADIUS Server, RADIUS Session Timeout, RADIUS Multiple MAC Address Formats, RADIUS DNS Host Name Support, RADIUS Start/Stop Accounting.
> † DHCP client requests and IP lease renewals are sent on the Ethernet interface only, not on Mesh links.
> ‡ Available on AP-4000M and AP-4900M only.

> ## Hardware Specifications

> ## Physical Specifications

> Dimensions (H x W x L) = 1.1 x 4.8 x 7.1 in (28 x 122 x 180 mm) plus additional antenna adaptor for AP-4900M
> Weight = .65 lb (.295 kg) for AP-4000/AP-4000M; .75 lb (.34 kg) for AP-4900M

> ## Electrical Specifications

> Voltage = 100 to 240 VAC (50-60 Hz)
> Current = 0.2 amp
> Power Consumption = <9 Watts (power supply)

> ## Environmental Specifications

> Operating = 0°C to 55°C (32°F to 131°F) @ 5 to 95% relative humidity, non-condensing at 5°C and 55°C
> Storage = -20°C to 85°C (-4°F to 185°F) @ 5 to 95% relative humidity, non-condensing at 5°C and 85°C.

> ## Ethernet Interface

> 10/100 Base-TX, RJ-45 female socket

> ## Serial Port Interface

> Standard RS-232C interface with DB-9, female connector

> ## Active Ethernet Interface

> Category 5, foiled, twisted pair cables must be used to ensure compliance with FCC Part 15, subpart B,
> Class B requirements

> Standard 802.3af pin assignments

> ## Available Channels

> Available channels vary based on radio, country, and frequency band. To verify which channels are available for your product:

> 1. Locate the product model number on the underside of your AP unit or on the unit's box.
> 2. Note the alphanumeric code following the number 8670. (e.g., 8670-EU)
> 3. See the following tables.
> NOTE: Country restrictions may apply. Please see Professional Installation.

> ## AP-4000/4000M Channels

> Radio | Frequency Band | Channel | Product Model Number
> --- | --- | --- | ---
> AU | AU2 | BR | CN | EU | EU2 | HK | JP | JP2 | SG | SK | TW | UK | US | US2 | WD
> 802.11b/g | - | 1 | 3 |  | 3 |  | See Channel Allocation by Country |  |  | 3 | 3 |  |  |  | See Channel Allocation by Country | 3 |  | See Channel Allocation by Country
> 2 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 3 | 3* |  | 3* |  |  |  | 3* | 3* |  |  |  | 3* |
> 4 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 5 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 6 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 7 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 8 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 9 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 10 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 11 | 3 |  | 3 |  |  |  | 3 | 3 |  |  |  | 3 |
> 12 |  |  | 3 |  |  |  | 3 | 3 |  |  |  |  |
> 13 |  |  | 3 |  |  |  | 3 | 3 |  |  |  |  |
> 14 |  |  |  |  |  |  | 3† | 3† |  |  |  |  |
> 802.11a | Lower | 34 |  |  |  |  |  |  | 3* |  |  |  |  |  |
> 36 | 3 | 3 | 3 |  | 3* |  |  | 3* |  |  |  |  | 3
> 38 |  |  |  |  |  |  | 3 |  |  |  |  |  |
> 40 | 3 | 3 | 3 |  | 3 |  |  | 3 |  |  |  |  | 3
> 42 |  |  |  |  |  |  | 3 |  |  |  |  |  |
> 44 | 3 | 3 | 3 |  | 3 |  |  | 3 |  |  |  |  | 3
> 46 |  |  |  |  |  |  | 3 |  |  |  |  |  |
> 48 | 3 | 3 | 3 |  | 3 |  |  | 3 |  |  |  |  | 3
> Middle | 52 | 3* | 3* |  |  | 3 |  |  | 3 |  |  |  | 3* | 3*
> 56 | 3 | 3 |  |  | 3 |  |  | 3 |  |  | 3* | 3 | 3
> 58 |  |  |  |  |  |  |  |  |  |  |  |  |
> 60 | 3 | 3 |  |  | 3 |  |  | 3 |  |  | 3 | 3 | 3
> 64 | 3 | 3 |  |  | 3 |  |  | 3 |  |  | 3 | 3 | 3
> High | 100 |  |  |  |  |  |  |  |  |  |  |  |  |
> 104 |  |  |  |  |  |  |  |  |  |  |  |  |
> 108 |  |  |  |  |  |  |  |  |  |  |  |  |
> 112 |  |  |  |  |  |  |  |  |  |  |  |  |
> 116 |  |  |  |  |  |  |  |  |  |  |  |  |
> 120 |  |  |  |  |  |  |  |  |  |  |  |  |
> 124 |  |  |  |  |  |  |  |  |  |  |  |  |
> 128 |  |  |  |  |  |  |  |  |  |  |  |  |
> 132 |  |  |  |  |  |  |  |  |  |  |  |  |
> 136 |  |  |  |  |  |  |  |  |  |  |  |  |
> 140 |  |  |  |  |  |  |  |  |  |  |  |  |
> Upper | 149 | 3 | 3 | 3 | 3* |  | 3* |  |  | 3* | 3* | 3 | 3 | 3
> 153 | 3 | 3 | 3 | 3 |  | 3 |  |  | 3 | 3 | 3 | 3 | 3
> 157 | 3 | 3 | 3 | 3 |  | 3 |  |  | 3 | 3 | 3 | 3 | 3
> 161 | 3 | 3 | 3 | 3 |  | 3 |  |  | 3 | 3 | 3 | 3 | 3
> ISM Band | 165 | 3 | 3 | 3 |  |  |  |  |  | 3 |  | 3 | 3 | 3

> * Default channel for radio.
> † Available for use only in 802.11b mode.

> ### Channel Allocation by Country

> Available channel bands in product models ending with -WD, -EU, and -UK depend on the selected country and mode of use (indoor/outdoor). See Frequency Bands for a list of channels in each band, and Frequency Bands by Country for a definition of allowed bands in each country.

> #### Frequency Bands

> Band | Supported Channels
> --- | ---
> Lower (L) | 36, 40, 44, 48
> Middle (M) | 52, 56, 60, 64
> High (H) | 100, 104, 108, 112, 116, 120, 124, 128, 132, 136, 140
> Upper (U) | 149, 153, 157, 161
> ISM | 165

> #### Frequency Bands by Country

> Country | Indoor/Outdoor | 802.11a Radio | 802.11b/g Radio | Country Identifier | .11d Country Code
> --- | --- | --- | --- | --- | ---
> Argentina | Indoor | M | 1 - 13 | AR1 | AR
> Australia | Indoor | L, M, U, ISM | 1 - 11 | AU1 | AU
> Outdoor | M, U, ISM | 1 - 11 | AU2 | AU
> Austria | Indoor | L, M, H | 1 - 13 | AT1 | AT
> Outdoor | H | 1 - 13 | AT2 | AT
> Belgium | Indoor | L, M, H | 1 - 13 | BE1 | BE
> Outdoor | H | 1 - 13 | BE2 | BE
> Bolivia | Indoor | L, M, U, ISM | 1 - 11 | BO1 | BO
> Outdoor | M, U, ISM | 1 - 11 | BO2 | BO
> Brazil | Indoor | L, U, ISM | 1 - 13 | BR1 | BR
> Outdoor | H, U, ISM | 1 - 13 | BR2 | BR
> Canada | Indoor | L, M, U, ISM | 1 - 11 | CA1 | CA
> Outdoor | M, U, ISM | 1 - 11 | CA2 | CA
> Chile | Indoor | L, M, U, ISM | 1 - 11 | CL1 | CL
> Outdoor | M, U, ISM | 1 - 11 | CL2 | CL
> China | Indoor/outdoor | U | 1 - 13 | CN1 | CN
> Cyprus | Indoor | L, M, H | 1 - 13 | CY1 | CY
> Outdoor | H | 1 - 13 | CY2 | CY
> Czech Republic | Indoor | L, M, H | 1 - 13 | CZ1 | CZ
> Outdoor | H | 1 - 13 | CZ2 | CZ
> Denmark | Indoor | L, M, H | 1 - 13 | DK1 | DK
> Outdoor | H | 1 - 13 | DK2 | DK
> El Salvador | Indoor | L, M, U, ISM | 1 - 11 | SV1 | SV
> Outdoor | M, U, ISM | 1 - 11 | SV2 | SV
> Estonia | Indoor | L, M, H | 1 - 13 | EE1 | EE
> Outdoor | H | 1 - 13 | EE2 | EE
> Finland | Indoor | L, M, H | 1 - 13 | FI1 | FI
> Outdoor | H | 1 - 13 | FI2 | FI
> France | Indoor | L, M, H | 1 - 13 | FR1 | FR
> Outdoor | H | 1 - 13 | FR2 | FR
> Germany | Indoor | L, M, H | 1 - 13 | DE1 | DE
> Outdoor | H | 1 - 13 | DE2 | DE
> Greece | Indoor | L, M, H | 1 - 13 | GR1 | GR
> Outdoor | H | 1 - 13 | GR2 | GR
> Guam | Indoor | L, M, U, ISM | 1 - 11 | GU1 | GU
> Outdoor | M, U, ISM | 1 - 11 | GU2 | GU
> Guatemala | Indoor | L, M, U, ISM | 1 - 11 | GT1 | GT
> Outdoor | M, U, ISM | 1 - 11 | GT2 | GT
> Honduras | Indoor | L, M, U, ISM | 1 - 11 | HN1 | HN
> Outdoor | M, U, ISM | 1 - 11 | HN2 | HN
> Hong Kong | Indoor | M, U, ISM | 1 - 11 | HK1 | HK
> Outdoor | U, ISM | 1 - 11 | HK2 | HK
> Hungary | Indoor | L, M, H | 1 - 13 | HU1 | HU
> Outdoor | H | 1 - 13 | HU2 | HU
> Iceland | Indoor | L, M, H | 1 - 13 | IS1 | IS
> Outdoor | H | 1 - 13 | IS2 | IS
> India | Indoor | N/A | N/A | IN1 | IN
> Ireland | Indoor | L, M, H | 1 - 13 | IE1 | IE
> Outdoor | H | 1 - 13 | IE2 | IE
> Italy | Indoor | L, M, H | 1 - 13 | IT1 | IT
> Outdoor | H | 1 - 13 | IT2 | IT
> Jamaica | Indoor | L, M, U, ISM | 1 - 11 | JM1 | JM
> Outdoor | M, U, ISM | 1 - 11 | JM2 | JM
> Latvia | Indoor | L, M, H | 1 - 13 | LV1 | LV
> Outdoor | H | 1 - 13 | LV2 | LV
> Liechtenstein | Indoor | L, M, H | 1 - 13 | LI1 | LI
> Outdoor | H | 1 - 13 | LI2 | LI
> Lithuania | Indoor | L, M, H | 1 - 13 | LT1 | LT
> Outdoor | H | 1 - 13 | LT2 | LT
> Luxembourg | Indoor | L, M, H | 1 - 13 | LU1 | LU
> Outdoor | H | 1 - 13 | LU2 | LU
> Malta | Indoor | L, M, H | 1 - 13 | MT1 | MT
> Outdoor | H | 1 - 13 | MT2 | MT
> Mexico | Indoor | L, M, U, ISM | 1 - 11 | MX1 | MX
> Outdoor | M, U, ISM | 1 - 11 | MX2 | MX
> Netherlands | Indoor | L, M, H | 1 - 13 | NL1 | NL
> Outdoor | H | 1 - 13 | NL2 | NL
> New Zealand | Indoor | L, M, U, ISM | 1 - 11 | NZ1 | NZ
> Outdoor | M, U, ISM | 1 - 11 | NZ2 | NZ
> Nicaragua | Indoor | L, M, U, ISM | 1 - 11 | NI1 | NI
> Outdoor | M, U, ISM | 1 - 11 | NI2 | NI
> Norway | Indoor | L, M, H | 1 - 13 | NO1 | NO
> Outdoor | H | 1 - 13 | NO2 | NO
> Papua New Guinea | Indoor | L, M, U, ISM | 1 - 11 | PG1 | PG
> Outdoor | M, U, ISM | 1 - 11 | PG2 | PG
> Poland | Indoor | L, M, H | 1 - 13 | PL1 | PL
> Outdoor | H | 1 - 13 | PL2 | PL
> Portugal | Indoor | L, M, H | 1 - 13 | PT1 | PT
> Outdoor | H | 1 - 13 | PT2 | PT
> Puerto Rico | Indoor | L, M, U, ISM | 1 - 11 | PR1 | PR
> Outdoor | M, U, ISM | 1 - 11 | PR2 | PR
> Russia | Indoor | L, M, H | 1 - 13 | RU1 | RU
> Outdoor | H | 1 - 13 | RU2 | RU
> Samoa | Indoor | L, M, U, ISM | 1 - 11 | WS1 | WS
> Outdoor | M, U, ISM | 1 - 11 | WS2 | WS
> Saudi Arabia | Indoor | L, U | 1 - 13 | SA1 | SA
> Singapore | Indoor | U, ISM | 1 - 11 | SG1 | SG
> Spain | Indoor | L, M, H | 1 - 13 | ES1 | ES
> Outdoor | H | 1 - 13 | ES2 | ES
> South Korea | Indoor/outdoor | U | 1 - 13 | KR1 | KR
> Sweden | Indoor | L, M, H | 1 - 13 | SE1 | SE
> Outdoor | H | 1 - 13 | SE2 | SE
> Switzerland | Indoor | L, M, H | 1 - 13 | CH1 | CH
> Outdoor | H | 1 - 13 | CH2 | CH
> Taiwan | Indoor | M, U, ISM | 1 - 11 | TW1 | TW
> Outdoor | U, ISM | 1 - 11 | TW2 | TW
> United Arab Emirates | Indoor | - | - | AE1 | AE
> United Kingdom | Indoor | L, M, H | 1 - 13 | GB1 | GB
> Outdoor | H | 1 - 13 | GB2 | GB

> ## AP-4900M Channels

> Channel availability in the AP-4900M depends on the operational mode. When operating in 802.11a-only, 802.11b-only, or 802.11b/g operational mode, the AP uses the channels in the following table. Additionally, when the AP-4900M's 802.11a radio is operating in 4.9 GHz Public Safety operational mode, the AP uses channels detailed in AP-4900M Channels (4.9 GHz Public Safety Mode).

> ### AP-4900M Channels (a/b/g Modes)

> Radio | Frequency Band | Channel | Available for use in 802.11a, 802.11b, or 802.11b/g modes
> --- | --- | --- | ---
> 802.11b/g | - | 1 | 3
> 2 | 3
> 3 | 3*
> 4 | 3
> 5 | 3
> 6 | 3
> 7 | 3
> 8 | 3
> 9 | 3
> 10 | 3
> 11 | 3
> 12 |
> 13 |
> 14 |
> 802.11a | Lower | 34 |
> 36 |
> 38 |
> 40 |
> 42 |
> 44 |
> 46 |
> 48 |
> Middle | 52 | 3*
> 56 | 3
> 58 |
> 60 | 3
> 64 | 3
> Upper | 149 | 3
> 153 | 3
> 157 | 3
> 161 | 3
> ISM Band | 165 | 3

> ### AP-4900M Channels (4.9 GHz Public Safety Mode)

> When operating in 4.9 GHz mode, channel availability depends on the selected frequency band.

> Channel | Frequency Band
> --- | ---
> 10 MHz | 20 MHz
> 10 | 3 |
> 15 |  |
> 20 | 3 | 3
> 25 |  |
> 30 | 3 | 3
> 35 |  |
> 40 | 3 | 3
> 45 |  |
> 50 | 3 | 3
> 55 |  |
> 60 | 3 | 3
> 65 |  |
> 70 | 3 | 3
> 75 |  |
> 80 | 3 | 3
> 85 |  |
> 90 | 3 |

www.proxim.com