## Interface Cable LEDs

Power / Ethernet Connection
Ethernet Link | Off Blink On | No link Ethernet activity Ethernet link established |  | RF Link | Off Blink On | No power (DC) No link Link established
GPS Transceiver Connection
RSL | Blink | The faster the blinking, the higher the RSL value. |  | GPS | Off Blink On | GPS disabled Enabled but not functioning Enabled & input okay

## Cable Descriptions

Cable #1 (50 meters, provided with radio)
Function Type Impedance Recommended cables Maximum Distance Connector type, radio end Connector type, power & Ethernet adapter end | Power (DC) and Ethernet connection Cat 5e, UV shielded 100 ohms 4 UTP, 24 AWG, UL rated 75 meters Note: The maximum length of the CAT5 cable allowed between the QuickBridge and the power adapter is 75 meters. This is also true for the cabling between the PC and the power adapter. Total length of the two cables should not exceed 100 meters. RJ-45 female, weatherized using weatherproof connector 8-pin DIN male connector with solder cup/cover or crimp pins to power & Ethernet adapter
Cable #2 (NOT provided with equipment; optional GPS receiver kit)
Function Type Connector type on radio end Maximum Length | GPS transceiver connection Serial cable, modified from vendor RJ-45 female, weatherized using weatherproof connector, with cover and O-ring over the connector 10 feet