> ## Technical Specifications

> Please see the following sections:

> - Part Numbers
> - Regulatory Approvals and Frequency Ranges
> - Integrated Antenna Specification
> - RF Modulation and Over-the-Air Rates
> - Wireless Protocol
> - Device Interface
> - Network Architecture Type
> - Receive Sensitivity
> - Maximum Throughput
> - Latency
> - Transmit Power Settings
> - Range Information
> - System Processor and Memory
> - Software Specification
> - Security
> - Management
> - Antenna
> - Status LEDs
> - Local Configuration Support
> - Compliance and Standards
> - Electrical
> - Dimensions
> - Weight
> - Environmental
> - Packaging Contents
> - MTBF
> - Warranty

> ## Part Numbers

> ## North America Region

> ### Model 2454-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 2454-BSUR-US-WORLD | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - US PSU -WORLD

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 2454-SUA-US-WORLD | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - US PSU -WORLD
> 2454-SUR-US-WORLD | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - US PSU -WORLD

> ### Model 5054-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 5054-BSUR-US | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - US PSU

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 5054-SUA-US | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - US PSU
> 5054-SUR-US | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - US PSU

> ## Europe and Middle East Regions

> ### Model 2454-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 2454-BSUR-EU | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - Europe PSU
> 2454-BSUR-UK | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - UK PSU

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 2454-SUA-EU | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - Europe PSU
> 2454-SUA-UK | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - UK PSU
> 2454-SUR-EU | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - Europe PSU
> 2454-SUR-UK | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - UK PSU

> ### Model 5054-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 5054-BSUR-EU | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - Europe PSU
> 5054-BSUR-UK | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - UK PSU

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 5054-SUA-EU | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - Europe PSU
> 5054-SUA-UK | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - UK PSU
> 5054-SUR-EU | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - Europe PSU
> 5054-SUR-UK | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - UK PSU

> ## Asia Pacific Region

> ### Model 2454-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 2454-BSUR-AU | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - Australia PSU
> 2454-BSUR-UK | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - UK PSU
> 2454-BSUR-US | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - US PSU
> 2454-BSUR-EU | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - Europe PSU
> 2454-BSUR-CN | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - China PSU
> 2454-BSUR-SK | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - South Korea PSU
> 2454-BSUR-US-WORLD | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - US/CAN PSU - WORLD

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 2454-SUA-AU | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - Australia PSU
> 2454-SUA-UK | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - UK PSU
> 2454-SUA-US | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - US PSU
> 2454-SUA-EU | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - EU PSU
> 2454-SUA-CN | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - China PSU
> 2454-SUA-SK | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - South Korea PSU
> 2454-SUA-US WORLD | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - US/CAN PSU - WORLD
> 2454-SUR-AU | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - Australia PSU
> 2454-SUR-UK | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - UK PSU
> 2454-SUR-US | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - US PSU
> 2454-SUR-EU | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - EU PSU
> 2454-SUR-CN | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - China PSU
> 2454-SUR-SK | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - South Korea PS
> 2454-SUR-US-WORLD | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 16-dBi Antenna - US/CAN PSU - WORLD

> ### Model 5054-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 5054-BSUR-AU | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - Australia PSU
> 5054-BSUR-UK | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - UK PSU
> 5054-BSUR-US | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - US PSU
> 5054-BSUR-EU | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - Europe PSU
> 5054-BSUR-US-WORLD | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - US/CAN PSU - WORLD

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 5054-SUA-AU | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - Australia PSU
> 5054-SUA-UK | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - UK PSU
> 5054-SUA-US | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - US PSU
> 5054-SUA-EU | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - EU PSU
> 5054-SUA-US-WORLD | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - US/CAN PSU - WORLD
> 5054-SUR-AU | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - Australia PSU
> 5054-SUR-UK | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - UK PSU
> 5054-SUR-US | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - US PSU
> 5054-SUR-EU | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - EU PSU
> 5054-SUR-US-WORLD | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - US/CAN PSU - WORLD

> ## Caribbean and Latin America Region

> ### Model 2454-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 2454-BSUR-US | Tsunami MP.11 Model 2454-R Base Station Unit with Type-N Connector - US PSU

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 2454-SUA-US | Tsunami MP.11 Model 2454-R Subscriber Unit with Type-N Connector - US PSU
> 2454-SUR-US | Tsunami MP.11 Model 2454-R Subscriber Unit with Integrated 23-dBi Antenna - US PSU

> ### Model 5054-R

> #### Base Station Unit

> Part Number | Description
> --- | ---
> 5054-BSUR-US | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - US PSU
> 5054-BSUR-BR | Tsunami MP.11 Model 5054-R Base Station Unit with Type-N Connector - Brazil PSU

> #### Subscriber Unit

> Part Number | Description
> --- | ---
> 5054-SUA-US | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - US PSU
> 5054-SUA-BR | Tsunami MP.11 Model 5054-R Subscriber Unit with Type-N Connector - Brazil PSU
> 5054-SUR-US | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - US PSU
> 5054-SUR-BR | Tsunami MP.11 Model 5054-R Subscriber Unit with Integrated 23-dBi Antenna - Brazil PSU

> ## Universal

> ### Accessories

> Part Number | Description
> --- | ---
> 848 274 163 | Surge Arrestor 0-3 GHz - Standard-N Female to Female
> 5054-SURGE | Surge Arrestor 5 GHz - Standard-N Female to Female
> 848 274 171 | 20 ft Low Loss Antenna Cable St-N - Male-Male LMR 200
> 848 332 789 | 20 ft Low Loss Antenna Cable St-N - Male-Male LMR 400
> 848 274 197 | 50 ft Low Loss Antenna Cable St-N - Male-Male LMR 400
> 848 274 205 | 75 ft Low Loss Antenna Cable St-N - Male-Male LMR 400
> 69828 | 6 ft Low Loss Antenna Cable St-N - Male-Male LMR 600
> 5054-LMR600-50 | 50 ft Low Loss Antenna Cable St-N - Male-Male LMR 600
> 70251 | PoE (Power over Ethernet) Surge Arrestor for Tsunami MP.11 and QuickBridge.11

> ### Outdoor Ethernet Cables

> Part Number | Description
> --- | ---
> 69819 | 25m outdoor, terminated CAT5 cable for Tsunami MP.11 or QB.11 with three RJ-45 and one weather-proof Ethernet port cap
> 69820 | 50m outdoor, terminated CAT5 cable for Tsunami MP.11 or QB.11 with three RJ-45 and one weather-proof Ethernet port cap
> 69821 | 75m outdoor, terminated CAT5 cable for Tsunami MP.11 or QB.11 with three RJ-45 and one weather-proof Ethernet port cap

> ### Power Injector

> Part Number | Description
> --- | ---
> 69823 | Spare Power DC Injector for Tsunami MP.11 or QB.11 (-R model ONLY)

> ### 2.4 GHz Antennas

> Part Number | Description
> --- | ---
> 848 515 722 | 5 dBi Omni-Directional Vehicle Antenna w/Integrated 250 cm cable
> 848 312 591 | 7 dBi Omni-Directional Base Station Antenna - St-N Female
> 848 515 698 | 10 dBi Omni-Directional Base Station Antenna - St-N Female
> 848 515 706 | 12 dBi Directional Wide Angle Antenna (120 degrees) - St-N Female
> 2411WA12-STN | 12 dBi Wide Angle Antenna with Integrated 2 m cable (st-N) Mountable on Window or Flat Surface
> 848 515 714 | 24 dBi Directional Antenna (Parabolic Grid) - St-N Female
> 2400-SA60-14 | 14dBi Directional sector antenna (60 degrees) 2.4GHz St-N Female

> ### 5 GHz Antennas

> Part Number | Description
> --- | ---
> 5054-PA-18 | 18 dBi Panel Antenna - St-N Female - 5.25 - 5.875 GHz
> 5054-PA-23 | 23 dBi Panel Antenna - St-N Female - 5.725 - 5.875 GHz
> 5054-OA-8 | 8 dBi Omni Directional Antenna - St-N Female - 5.47-5.850 GHz
> 5054-OA-10 | 10 dBi Omni Directional Antenna - St-N Female - 5.47-5.850 GHz
> 5054-SA120-14 | 14 dBi Sector Antenna - St-N Female - 5.25-5.850 GHz - 120 degrees
> 5054-SA60-17 | 17 dBi Sector Antenna - St-N Female - 5.25-5.850 GHz - 60 degrees

> ## Regulatory Approvals and Frequency Ranges

> ## Model 2454-R Regulatory Approval and Frequency Ranges

> Region/Country | Country | GHz | Number of Channels | Certification
> --- | --- | --- | --- | ---
> 5 MHz | 10 MHz | 20 MHz
> North America | USA | 2.40 - 2.4835 | 11 | Up to 11 | Up to 11 | Yes
> 2.40 - 2.472 | 13 | Up to 13 | Up to 13 | Yes
> Canada | 2.40 - 2.4835 | 11 | Up to 11 | Up to 11 | Yes
> 2.40 - 2.472 | 13 | Up to 13 | Up to 13 | Yes
> Mexico | 2.40 - 2.4835 | 11 | Up to 11 | Up to 11 | Yes
> 2.40 - 2.472 | 13 | Up to 13 | Up to 13 | Yes
> EU Countries | Austria | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Belgium | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Cyprus | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Czech Republic | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Denmark | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Estonia | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Finland | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> France | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Germany | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Greece | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Hungary | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Ireland | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Italy | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Latvia | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Luxemburg | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Lithuania | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Malta | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Netherlands | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Poland | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Portugal | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Spain | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Sweden | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Slovakia | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Slovenia | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> United Kingdom | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Other European Countries | Iceland | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Liechtenstein | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Norway | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Switzerland | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> South America | Brazil | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | In Process
> APAC | New Zealand | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Japan | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Hong Kong | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> S. Korea | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> China | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes
> Taiwan | 2.40 - 2.4835 | 13 | Up to 13 | Up to 13 | Yes

> ## Model 5054-R Regulatory Approval and Frequency Ranges

> Region/Country | Country | GHz | Number of Channels | Certification
> --- | --- | --- | --- | ---
> 5 MHz | 10 MHz | 20 MHz
> North America | USA | 5.25 - 5.35 | Up to 15 | Up to 7 | Up to 3 | Yes
> 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5
> Canada | 5.25 - 5.35 | Up to 15 | Up to 7 | Up to 3 | Yes
> 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5
> Mexico | 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5 | Yes
> EU Countries | Austria | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Belgium | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Cyprus | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Czech Republic | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Denmark | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Estonia | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Finland | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> France | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Germany | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Greece | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Hungary | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Ireland | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> 5.725 - 5.85 | Up to 23 | Up to 11 | Up to 4
> Italy | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Latvia | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Lithuania | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Luxemburg | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Malta | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Netherlands | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Poland | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Portugal | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Slovakia | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Slovenia | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Spain | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Sweden | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> United Kingdom | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> 5.725 - 5.85 | Up to 23 | Up to 11 | Up to 4
> Other European Countries | Iceland | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Liechtenstein | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Norway | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> Russia | 5.15 - 5.85 | Up to 141 | Up to 71 | Up to 36 | In Process
> Switzerland | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> South America | Argentina | 5.25 - 5.35 | Up to 9 | Up to 5 | Up to 3 | Yes
> 5.725 - 5.85 | Up to 19 | Up to 10 | Up to 5
> Brazil | 5.47 - 5.70 | Up to 46 | Up to 23 | Up to 11 | Yes
> 5.725 - 5.85 | Up to 19 | Up to 10 | Up to 5
> Colombia | 5.25 - 5.35 | Up to 15 | Up to 7 | Up to 3 | Yes
> 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5
> APAC | Australia | 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5 | Yes
> China | 5.725 - 5.85 | Up to 17 | Up to 9 | Up to 5 | Yes
> Hong Kong | 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5 | Yes
> India | 5.15 - 5.35 | Up to 32 | Up to 16 | Up to 7 | In Process
> 5.725 - 5.85 | Up to 17 | Up to 9 | Up to 5
> New Zealand | 5.725 - 5.85 | Up to 21 | Up to 11 | Up to 5 | Yes
> S. Korea | 5.725 - 5.85 | Up to 17 | Up to 9 | Up to 5 | Yes
> Singapore | 5.15 - 5.25 | Up to 13 | Up to 7 | Up to 4 | In Process
> 5.725 - 5.85 | Up to 17 | Up to 9 | Up to 5
> Taiwan | 5.25 - 5.35 | Up to 15 | Up to 7 | Up to 3 | Yes
> 5.725 - 5.85 | Up to 17 | Up to 9 | Up to 5

> ## Integrated Antenna Specification

> ## Model 2454-R

> ### Subscriber Unit with Integrated 16-dBi Antenna

> Feature | Specification
> --- | ---
> Part Number | 2454-SUR-xx
> Frequency range | 2.4 to 2.5 GHz
> Nominal Impedance | 50 Ohms
> Gain | 16 dBi
> Front-to-Back Ratio | 25 dB
> HPBW/vertical | 22 degrees
> HPBW/horizontal | 15 degrees
> Cross Polarization | 20 dB
> Power handling | 1 W
> VSWR | 1.5 : 1 Max

> ## Model 5054-R

> ### Subscriber Unit with Integrated 23-dBi Antenna

> Feature | Specification
> --- | ---
> Part Number | 5054-SUR-xx
> Frequency range | 5250 - 5875 MHz
> Nominal Impedance | 50 ohms
> Gain | 23 dBi
> Front-to-Back Ratio | 35 dB
> HPBW/vertical | 9 degrees
> HPBW/horizontal | 9 degrees
> Cross Polarization | 23 dB
> Power handling | 1 W (cw)
> VSWR | 2.0 : 1 Max

> ## RF Modulation and Over-the-Air Rates

> ## Model 2454-R and 5054-R OFDM (Orthogonal Frequency Division Multiplexing)

> - Maximum Packet Size 1522 Bytes
> - Modulation Rates:

> Modulation | Rate
> --- | ---
> 20 MHz Channels | 10 MHz Channels | 5 MHz Channels
> BPSK | 6 and 9 Mbps | 3 and 4.5 Mbps | 2.25 and 1.5 Mbps
> QPSK | 12 and 18 Mbps | 6 and 9 Mbps | 3 and 4.5 Mbps
> 16-QAM | 24 and 36 Mbps | 12 and 18 Mbps | 6 and 9 Mbps

> ## Wireless Protocol

> - Worp (Wireless Outdoor Router Protocol)

> ## Device Interface

> - Ethernet: Auto-sensing 10/100BASE-TX Ethernet
> - Antenna Connector for BSU and SU with Type-N Connector: Standard Type-N Female

> ## Network Architecture Type

> - Infrastructure

> ## Receive Sensitivity

> - BER=10-6

> ## 2454-R/5054-R

> Modulation | 40 MHz Channels Turbo Mode (US only) | 20 MHz Channels Standard Mode | 10 MHz Channels Standard Mode | 5 MHz Channels Standard Mode
> 64QAM ¾ | -66 dBm @108Mbps | -69 dBm @54Mbps | -72 dBm @36Mbps | -75 dBm @18Mbps
> 64QAM ½ | -68 dBm @96Mbps | -72 dBm @48Mbps | -75 dBm @24Mbps | -78 dBm @12Mbps
> 16QAM ¾ | -75dBm @72Mbps | -77 dBm @36Mbps | -80 dBm @18Mbps | -83 dBm @9Mbps
> 16QAM ½ | -78dBm @48Mbps | -80 dBm @24Mbps | -83 dBm @12Mbps | -86 dBm @6Mbps
> QPSK ¾ | -81dBm @36Mbps | -83 dBm @18Mbps | -86 dBm @9Mbps | -89 dBm @4.5Mbps
> QPSK ½ | -83 dBm @24Mbps | -86 dBm @12Mbps | -89 dBm @6Mbps | 92 dBm @3Mbps
> BPSK ¾ | -84 dBm @18Mbps | -87 dBm @9Mbps | -90 dBm @4.5Mbps | -93 dBm @2.25Mbps
> BPSK ½ | -85 dBm @12Mbps | -88 dBm @6Mbps | -91 dBm @3Mbps | -94 dBm @1.5Mbps

> ## Maximum Throughput

> ## 2454-R

> Data Rate | 20 MHz Channels | 10 MHz Channels | 5 MHz Channels Standard Mode
> --- | --- | --- | ---
> 54 Mbps | 30 Mbps | - | -
> 48 Mbps | 28 Mbps | - | -
> 36 Mbps | 18 Mbps | - | -
> 24 Mbps | 14 Mbps | - | -
> 18 Mbps | 12 Mbps | 12 Mbps | -
> 12 Mbps | 9 Mbps | 9 Mbps | -
> 9 Mbps | 7 Mbps | 7 Mbps | 6.8 Mbps
> 6 Mbps | 5 Mbps | 5 Mbps | 5 Mbps
> 4.5 Mbps | - | 4 Mbps | 4 Mbps
> 3 Mbps | - | 2 Mbps | 2.7 Mbps
> 2.25 Mbps | - | - | 2 Mbps
> 1 Mbps | - | - | 1.4 Mbps

> Note: Maximum-throughput data with release 2.3, as measured with test equipment under controlled lab condi- tions and best performing packet size. In some instances, data compression yields throughput equal to the configured data rate. Actual throughput performance in the field may vary.

> ## 5054-R

> Data Rate | 40 MHz Channels (US Only) | 20 MHz Channels | 10 MHz Channels | 5 MHz Channels Standard Mode
> --- | --- | --- | --- | ---
> 108 Mbps Turbo 54 | 31 Mbps | - | - | -
> 96 Mbps Turbo 48 | 28 Mbps | - | - | -
> 72 Mbps Turbo 36 | 28 Mbps | - | - | -
> 48 Mbps Turbo 24 | 28 Mbps | - | - | -
> 36 Mbps Turbo 18 | 24 Mbps | - | - | -
> 24 Mbps Turbo 12 | 19 Mbps | - | - | -
> 54 Mbps | - | 29 Mbps | - | -
> 48 Mbps | - | 27 Mbps | - | -
> 36 Mbps | - | 22 Mbps | - | -
> 24 Mbps | - | 16 Mbps | 16 Mbps | -
> 18 Mbps | - | 13 Mbps | 13 Mbps | -
> 12 Mbps | - | 9 Mbps | 9 Mbps | -
> 9 Mbps | - | 7 Mbps | 7 Mbps | 7 Mbps
> 6 Mbps | - | 5 Mbps | 5 Mbps | 4.7 Mbps
> 4.5 Mbps | - | - | 3.6 Mbps | 3.8 Mbps
> 3 Mbps | - | - | 2.4 Mbps | 2.7 Mbps
> 2.25 Mbps | - | - | - | 2 Mbps
> 1 Mbps | - | - | - | 1.2 Mbps

> Note: Maximum-throughput data with release 2.3, as measured with test equipment under controlled lab condi- tions and best performing packet size. In some instances, data compression yields throughput equal to the configured data rate. Actual throughput performance in the field may vary.

> ## Latency

> - < 10ms typical at maximum throughput (as measured with test equipment under controlled lab conditions and best performing packet size)

> ## Transmit Power Settings

> ## Model 2454-R

> - Output Power Attenuation: 0 - 18dB, in 3dB steps
> - Output Power Values will have a tolerance of +- 1.5 dB

> Frequency | 6-24 Mbps @ 20 MHz 16QAM ½; QPSK ¾; QPSK ½; BPSK ¾; BPSK ½ | 36 Mbps @ 20 MHz 16QAM ¾ | 48 Mbps @ 20 MHz 64QAM ½ | 54 Mbps @ 20 MHz 64QAM ¾
> --- | --- | --- | --- | ---
> 2.400-2.483 GHz | 16 dBm | 16 dBm | 14 dBm | 13 dBm

> ## Model 5054-R

> - Output Power Attenuation: 0 - 18dB, in 3dB steps
> - Output Power Values will have a tolerance of +- 1.5 dB

> Frequency | 6-24 Mbps @ 20 MHz 16QAM ½; QPSK ¾; QPSK ½; BPSK ¾; BPSK ½ | 36 Mbps @ 20 MHz 16QAM ¾ | 48 Mbps @ 20 MHz 64QAM ½ | 54 Mbps @ 20 MHz 64QAM ¾
> --- | --- | --- | --- | ---
> 5.15-5.35 GHz | 15 dBm | 13 dBm | 12 dBm | 11 dBm
> 5.47-5.725 GHz | 16 dBm | 13 dBm | 12 dBm | 11 dBm
> 5.725-5.850 GHz | 16 dBm | 13 dBm | 12 dBm | 11 dBm

> ## Range Information

> ## Model 2454-R

> ### Integrated Antenna

> Frequency | 36 Mbps | 6 Mbps
> --- | --- | ---
> 2.4-2.4835GHz (US) | 2.1mi/3.4km | 6.9mi/11.1km
> 2.4-2.8 GHz (ETSI) | 0.7mi/1.1km | 2.6mi/4.2km

> ### External Antenna

> Frequency | 36 Mbps | 6 Mbps
> --- | --- | ---
> 2.4-2.4835GHz (US) | 3.4mi/5.5km | 11.4mi/18.3km
> 2.4-2.8 GHz (ETSI) | 0.7mi/1.1km | 2.6mi/4.2km

> ## Model 5054-R

> ### Integrated Antenna

> Frequency | 36 Mbps | 6 Mbps
> --- | --- | ---
> 5.15-5.35 GHz (US) | 1.2mi/2.0km | 3.0mi/4.8km
> 5.47-5.7GHz (ETSI) | 1.1mi/1.8km | 3.1mi/5.0km
> 5.725-5.850 (US) | 2.1mi/3.8km | 6.4mi/10.3km

> ### External Antenna

> Frequency | 36 Mbps | 6 Mbps
> --- | --- | ---
> 5.15-5.35 GHz (US) | 1.2mi/2.0km | 3.2mi/5.1km
> 5.47-5.7GHz (ETSI) | 1.1mi/1.8km | 3.1mi/5.0km
> 5.725-5.850 (US) | 4.1mi/6.6km | 12.5mi/20.1km

> ## Notes

> Note the following:

> - PMP configuration using USA regulations for L and U bands, ETSI regulations for M bands
> - Clear LOS
> - 99.995% availability
> - Sector antenna (17dBi, 60-degrees) at BSU with short 1dB jumper cable
> - Fade margin minimum of 10dB to 2 miles, 0.2dB additional fade margin for every 0.1 mile to 15dB
> - Predicted availability >99.990% (one-way) for all configurations
> - Distance calculations for 5 and 10 MHz channels are comparable for ETSI regulatory domains. Proper TPC settings (3 and 6dB) respectively, should be set to meet power density rules. Increased distances are possible in the US with proper link engineering.

> ## System Processor and Memory

> - 166MHz Motorola 8241 processor
> - 16 Mbytes RAM
> - 8 Mbytes FLASH

> ## Software Specification

> ## Base Station and Subscriber Units

> - Miscellaneous
> - WORP protocol
> - Dynamic Data Rate Selection
> - Transmit Power Control
> - Antenna Alignment
> - Integrity Check for Software Upload
> - 5, 10, and 20MHz channels
> - Satellite Density
> - Dynamic Frequency Selection
> - Redundancy
> - Spanning Tree (802.1D)
> - Bridging and Routing
> - Bridge (802.1d)
> - IP/ RIPv1 (RFC 1058)
> - IP/ RIPv2 (RFC 1388)
> - CIDR (RFC 1519)
> - ICMP (RFC 792)
> - IP (RFC 791)
> - ARP (RFC 826)
> - Filtering
> - Ethernet protocol (Ethertype)
> - Static MAC
> - Storm threshold
> - IP address
> - Broadcast protocol
> - Services
> - DHCP Server (RFC 2131)
> - DHCP Client (RFC 2131)
> - Bi-Directional Bandwidth Control
> - VLAN
> - 802.1Q
> - Security Features
> - MAC Authentication
> - Radius MAC Access Control
> - WEP/AES-OCB encryption
> - RADIUS (RFC 2138)
> - Mobility
> - Subscriber Unit Roaming

> ## Base Station Unit

> - Filtering
> - Intra Cell Blocking

> ## Subscriber Units

> - Services
> - NAT (RFC 3022)
> - DHCP Relay (RFC 2131)

> ## Security

> - WORP provides critical feature support for secure long-range wireless deployments in unlicensed frequency spectrum.
> - MD5 (embedded in WORP) authentication between BSU and SU.
> - Filter based on packet information such as unicast/multicast/ broadcast MAC or IP.
> - Secure "over the air encryption" with WEP, WEP+, and AES, and AES-CCB.
> - Authentication via Radius
> - Intracell blocking allows the BSU to act as the central policy enforcer for SU to SU communications.

> ## Management

> - SU/BSU statistics
> - Link Test
> - Temperature logging
> - SNMPv1/v2 RFC 1157
> - SNMP v2c (RFC 1907)
> - HTTP Server (RFC 2616)
> - Telnet (RFC 855)
> - TFTP client (RFC 783)
> - CLI
> - MIB-II (RFC 1213)
> - Ethernet-like MIB (RFC 1643)
> - Bridge MIB (RFC 1493)
> - 802.3MAU (RFC 2668)
> - 802.11 MIB
> - Remote reboot (reload) or reset to factory default via power injector
> - Private MIB
> - Orinoco MIB

> ## Antenna

> - Audible tone
> - CLI output

> ## Status LEDs

> - Two indicators on the RJ-45 connector to indicate power, wireless traffic, and Ethernet traffic

> ## Local Configuration Support

> - RS-232 Serial port
> - RJ11 port built-into the unit
> - DB9 Female via a converter (included)

> ## Compliance and Standards

> ## Safety

> - UL: 60950, UL50
> - CSA: 22.2 No. 60950-00
> - IEC: 60950 3rd Ed (1999)

> ## Radio Approvals

> - USA: FCC 15.107, 15-109; 15-203-15.205, 15.207, 15.209; 15.247; 15.401-15.407
> - Canada: RSS-102; RSS-210; ICES-003
> - Europe (ETSI): EN 301.893; EN 300.328; EN 301.489-1; EN 301.489-17; EN 300-440; EN50371
> - ARIB: STD-T71, STD 33, STD 66

> ## EMI and Susceptibility (Class B)

> - USA: FCC Part 15.107
> - Canada: ICES-003

> ## Water and Dust Proof

> - NEMA4/IP56

> ## Electrical

> ## 5054-R / 2454-R POE Power Injector

> - Custom Power over Ethernet (802.3af compatible)
> - Input: Voltage 110 to 250 VAC (47-63Hz)
> - Output: 48V @ 420mA MAX (injected into the Cat-5 Cable)
> - Pin for Remote reboot (reload) or reset to factory default

> ## 5054-R / 2454-R Outdoor Radio Unit

> - Power Consumption: 7.5W typical. Up to 20 Watts across full operating temperature range.
> - Input: Voltage 42 to 60 VDC

> ## Dimensions

> ## Base Station and Subscriber Unit

> - Packaged: 14.57 in x 13.70 in x 8.19 in (370 mm x 348 mm x 208 mm)

> ## Base Station and Subscriber Unit with Type-N Connector

> - Unpackaged: 10.5 in x 10.5 in x 3.25 in (267 mm x 267 mm x 83 mm)

> ## Subscriber Unit with Integrated 23-dBi Antenna

> - Unpackaged: 12.60 in x 12.60 in x 3.50 in (320 mm x 320 mm x 89 mm)

> ## Weight

> ## Base Station and Subscriber Unit with Type-N Connector

> - Packaged weight: 9.2 lbs (4.2 kg)
> - Unpackaged weight: 5.5 lbs (2.49 kg) Unit-only, .45 lbs (.20 kg) for power supply

> ## Subscriber Unit with Integrated 23-dBi or 16-dBi Antenna

> - Packaged weight: 10.1 lbs (4.6 kg)
> - Unpackaged weight: 6.0 lbs (2.72 kg) Unit-only, .45 lbs (.20 kg) for power supply

> ## Environmental

> ## Operating

> - -33º to 60ºC (-27.5º to 140º Fahrenheit)
> - 100% humidity
> - Wind loading: 125 mph

> ## Storage

> - -55º to 80ºC (-41º to 176º Fahrenheit)
> - 100% humidity

> ## Packaging Contents

> - One Tsunami MP.11 Model 2454-R or 5054-R Base Station or Subscriber Unit
> - One wall/ pole mounting bracket
> - One Power-Over-Ethernet injector for Model 2454-R or 5054-R
> - One country specific power cord
> - One Ethernet cable weather-proof plug
> - One Documentation and Software CD-ROM

> ## MTBF

> - 100,000 hours

> ## Warranty

> - One year